(module OWN_DC-DC (layer F.Cu) (tedit 0)
  (fp_text reference Ref** (at 0 0) (layer F.SilkS)
    (effects (font (size 1.27 1.27) (thickness 0.15)))
  )
  (fp_text value Val** (at 0 0) (layer F.SilkS)
    (effects (font (size 1.27 1.27) (thickness 0.15)))
  )
  (fp_line (start -17.145 -10.795) (end -17.145 0.635) (layer F.SilkS) (width 0.127))
  (fp_line (start -17.145 0.635) (end 0.635 0.635) (layer F.SilkS) (width 0.127))
  (fp_line (start 0.635 0.635) (end 0.635 -10.795) (layer F.SilkS) (width 0.127))
  (fp_line (start 0.635 -10.795) (end -17.145 -10.795) (layer F.SilkS) (width 0.127))
  (fp_line (start -17.145 -10.795) (end -17.145 0.635) (layer B.SilkS) (width 0.127))
  (fp_line (start -17.145 -10.795) (end 0.635 -10.795) (layer B.SilkS) (width 0.127))
  (fp_line (start 0.635 0.635) (end 0.635 -10.795) (layer B.SilkS) (width 0.127))
  (fp_line (start 0.635 0.635) (end -17.145 0.635) (layer B.SilkS) (width 0.127))
  (fp_text user +IN (at -15.24 -8.89) (layer F.SilkS)
    (effects (font (size 1.2065 1.2065) (thickness 0.1016)) (justify left bottom))
  )
  (fp_text user OUT+ (at -1.27 -8.89) (layer F.SilkS)
    (effects (font (size 1.2065 1.2065) (thickness 0.1016)) (justify right bottom))
  )
  (fp_text user GND (at -8.255 0) (layer F.SilkS)
    (effects (font (size 1.2065 1.2065) (thickness 0.1016)) (justify bottom))
  )
  (fp_text user +IN (at -15.24 -8.89) (layer B.SilkS)
    (effects (font (size 1.2065 1.2065) (thickness 0.1016)) (justify right bottom mirror))
  )
  (fp_text user OUT+ (at -1.27 -8.89) (layer B.SilkS)
    (effects (font (size 1.2065 1.2065) (thickness 0.1016)) (justify left bottom mirror))
  )
  (fp_text user GND (at -8.255 0) (layer B.SilkS)
    (effects (font (size 1.2065 1.2065) (thickness 0.1016)) (justify bottom mirror))
  )
  (pad IN+ thru_hole rect (at -15.875 -9.525) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad IN- thru_hole rect (at -15.875 -0.635) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad OUT+ thru_hole rect (at -0.635 -9.525) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad OUT- thru_hole rect (at -0.635 -0.635) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
